{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":47,"n_cols":14,"rows_kept":47,"cut":false,"hidden":false,"merged":[]}
[null,"Start Date:",{"$f":"MIN(A8:A1048576)","v":"2018-01-01"},null,"Employee Name:","Excel Crib",null,"How to use the spreadsheet in 3 steps"]
[null,"End Date:",{"$f":"MAX(A8:A1048576)","v":"2018-01-12"},null,"Employee No:","E355"]
[null,null,null,null,null,null,null,"Step 1.  When a security warning appears, press 'Enable Content' (see below picture) and then trust "]
["Timesheet",null,null,null,"Total number of hours:",{"$f":"SUM(F8:F1048576)","v":85},null,"    the document by clicking yes. It is a common warning when a spreadsheet uses a VBA programming. "]
[]
[]
["Date","Item Code","Item Description","Start Time","End Time","No. of Hours"]
["2018-01-01",15764,"Design of level 1 columns","07:00:00","08:30:00",{"$f":"(E8-D8)*1440/60","v":1.5}]
[null,22007,"Level 2 slab design","08:30:00","12:30:00",{"$f":"(E9-D9)*1440/60","v":4.0000000000000009}]
[null,24509,"Checking of rebar","12:30:00","14:30:00",1.999999999999998]
[null,15764,"Design of level 2 columns","14:30:00","15:30:00",1.0000000000000018]
["2018-01-02",15764,"Design of level 1 columns","07:00:00","08:30:00",{"$f":"(E12-D12)*1440/60","v":1.5}]
[null,22007,"Level 2 slab design","08:30:00","12:30:00",{"$f":"(E13-D13)*1440/60","v":4.0000000000000009}]
[null,24509,"Checking of rebar","12:30:00","14:30:00",1.999999999999998]
[null,15764,"Design of level 2 columns","14:30:00","15:30:00",1.0000000000000018]
["2018-01-03",15764,"Design of level 1 columns","07:00:00","08:30:00",{"$f":"(E16-D16)*1440/60","v":1.5}]
[null,22007,"Level 2 slab design","08:30:00","12:30:00",{"$f":"(E17-D17)*1440/60","v":4.0000000000000009}]
[null,24509,"Checking of rebar","12:30:00","14:30:00",1.999999999999998]
[null,15764,"Design of level 2 columns","14:30:00","15:30:00",1.0000000000000018]
["2018-01-04",15764,"Design of level 1 columns","07:00:00","08:30:00",{"$f":"(E20-D20)*1440/60","v":1.5}]
[null,22007,"Level 2 slab design","08:30:00","12:30:00",{"$f":"(E21-D21)*1440/60","v":4.0000000000000009}]
[null,24509,"Checking of rebar","12:30:00","14:30:00",1.999999999999998]
[null,15764,"Design of level 2 columns","14:30:00","15:30:00",1.0000000000000018]
["2018-01-05",15764,"Design of level 1 columns","07:00:00","08:30:00",{"$f":"(E24-D24)*1440/60","v":1.5}]
[null,22007,"Level 2 slab design","08:30:00","12:30:00",{"$f":"(E25-D25)*1440/60","v":4.0000000000000009}]
[null,24509,"Checking of rebar","12:30:00","14:30:00",1.999999999999998]
[null,15764,"Design of level 2 columns","14:30:00","15:30:00",1.0000000000000018]
["2018-01-08",15764,"Design of level 1 columns","07:00:00","08:30:00",{"$f":"(E28-D28)*1440/60","v":1.5},null,"Step 2.  Input all cells in blue texts. Add/delete rows and adjust cells as necessary."]
[null,22007,"Level 2 slab design","08:30:00","12:30:00",{"$f":"(E29-D29)*1440/60","v":4.0000000000000009}]
[null,24509,"Checking of rebar","12:30:00","14:30:00",1.999999999999998,null,"Step 3. Press 'Print' button."]
[null,15764,"Design of level 2 columns","14:30:00","15:30:00",1.0000000000000018]
["2018-01-09",15764,"Design of level 1 columns","07:00:00","08:30:00",{"$f":"(E32-D32)*1440/60","v":1.5},null,"This is version 1.0, please visit our website",null,null,null,"www.excelcrib.com",null,"to get the most updated spreadsheet."]
[null,22007,"Level 2 slab design","08:30:00","12:30:00",{"$f":"(E33-D33)*1440/60","v":4.0000000000000009},null,"Feel free to ask us questions."]
[null,24509,"Checking of rebar","12:30:00","14:30:00",1.999999999999998]
[null,15764,"Design of level 2 columns","14:30:00","15:30:00",1.0000000000000018]
["2018-01-10",15764,"Design of level 1 columns","07:00:00","08:30:00",{"$f":"(E36-D36)*1440/60","v":1.5}]
[null,22007,"Level 2 slab design","08:30:00","12:30:00",{"$f":"(E37-D37)*1440/60","v":4.0000000000000009}]
[null,24509,"Checking of rebar","12:30:00","14:30:00",1.999999999999998]
[null,15764,"Design of level 2 columns","14:30:00","15:30:00",1.0000000000000018]
["2018-01-11",15764,"Design of level 1 columns","07:00:00","08:30:00",{"$f":"(E40-D40)*1440/60","v":1.5}]
[null,22007,"Level 2 slab design","08:30:00","12:30:00",{"$f":"(E41-D41)*1440/60","v":4.0000000000000009}]
[null,24509,"Checking of rebar","12:30:00","14:30:00",1.999999999999998]
[null,15764,"Design of level 2 columns","14:30:00","15:30:00",1.0000000000000018]
["2018-01-12",15764,"Design of level 1 columns","07:00:00","08:30:00",{"$f":"(E44-D44)*1440/60","v":1.5}]
[null,22007,"Level 2 slab design","08:30:00","12:30:00",{"$f":"(E45-D45)*1440/60","v":4.0000000000000009}]
[null,24509,"Checking of rebar","12:30:00","14:30:00",1.999999999999998]
[null,15764,"Design of level 2 columns","14:30:00","15:30:00",1.0000000000000018]